Unfiltered SIL Load Rig data in CA, run for 30 seconds load motor off, then 30 second with load motor on

Unfiltered ATP Load Rig data in UT, run with Load motor on for a few seconds, then off for the remainder of time.

Unfiltered ATP DEV data in UT, run for short duration with load motor off, then on, and off again.